{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["ARTIKEL"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"ARTIKEL","index":0,"n_rows":291,"n_cols":15,"rows_kept":291,"cut":false,"hidden":false,"merged":[]}
["arArtikelnr","arArtikelnr neu","arKurztext1","arKurztext2","arMengeneinheit","arPreisEinheit","arPreisEuro","arVerpackungsmenge","hwHwgr","rgRgr","ltLangtextnr","arMatchcode","arEANNummer","arKatalogseite","arVerarbKz"]
["ADK","\"\"","Abdeckkappe","","Stck",0,"","","","","","KAPPE","","","N"]
["ALS191","\"\"","Allergiker-Set bestehend aus","1 Wasserkasette und 19 Staubfilter","Stck",0,"","","","","ALS","ALLERGIKERSET","","","N"]
["C1-1200-10","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1200 mm, Länge: 760 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1200-11","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1200 mm, Länge: 836 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1200-12","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1200 mm, Länge: 912 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1200-13","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1200 mm, Länge: 988 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1200-14","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1200 mm, Länge: 1064 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1200-15","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1200 mm, Länge: 1140 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1200-16","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1200 mm, Länge: 1216 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1200-17","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1200 mm, Länge: 1292 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1200-18","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1200 mm, Länge: 1368 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1200-19","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1200 mm, Länge: 1444 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1200-20","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1200 mm, Länge: 1520 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1200-4","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1200 mm, Länge: 304 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1200-5","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1200 mm, Länge: 380 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1200-6","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1200 mm, Länge: 456 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1200-7","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1200 mm, Länge: 532 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1200-8","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1200 mm, Länge: 608 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1200-9","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1200 mm, Länge: 684 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1600-10","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1600 mm, Länge: 760 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1600-11","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1600 mm, Länge: 836 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1600-12","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1600 mm, Länge: 912 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1600-13","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1600 mm, Länge: 988 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1600-14","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1600 mm, Länge: 1064 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1600-15","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1600 mm, Länge: 1140 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1600-16","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1600 mm, Länge: 1216 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1600-17","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1600 mm, Länge: 1292 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1600-18","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1600 mm, Länge: 1368 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1600-19","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1600 mm, Länge: 1444 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1600-20","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1600 mm, Länge: 1520 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1600-4","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1600 mm, Länge: 304 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1600-5","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1600 mm, Länge: 380 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1600-6","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1600 mm, Länge: 456 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1600-7","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1600 mm, Länge: 532 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1600-8","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1600 mm, Länge: 608 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1600-9","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1600 mm, Länge: 684 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1800-10","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1800 mm, Länge: 760 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1800-11","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1800 mm, Länge: 836 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1800-12","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1800 mm, Länge: 912 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1800-13","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1800 mm, Länge: 988 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1800-14","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1800 mm, Länge: 1064 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1800-15","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1800 mm, Länge: 1140 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1800-16","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1800 mm, Länge: 1216 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1800-17","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1800 mm, Länge: 1292 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1800-18","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1800 mm, Länge: 1368 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1800-19","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1800 mm, Länge: 1444 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1800-20","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1800 mm, Länge: 1520 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1800-4","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1800 mm, Länge: 304 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1800-5","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1800 mm, Länge: 380 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1800-6","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1800 mm, Länge: 456 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1800-7","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1800 mm, Länge: 532 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1800-8","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1800 mm, Länge: 608 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-1800-9","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 1800 mm, Länge: 684 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-2000-10","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 2000 mm, Länge: 760 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-2000-11","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 2000 mm, Länge: 836 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-2000-12","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 2000 mm, Länge: 912 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-2000-13","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 2000 mm, Länge: 988 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-2000-14","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 2000 mm, Länge: 1064 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-2000-15","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 2000 mm, Länge: 1140 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-2000-16","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 2000 mm, Länge: 1216 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-2000-17","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 2000 mm, Länge: 1292 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-2000-18","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 2000 mm, Länge: 1368 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-2000-19","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 2000 mm, Länge: 1444 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-2000-20","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 2000 mm, Länge: 1520 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-2000-4","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 2000 mm, Länge: 304 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-2000-5","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 2000 mm, Länge: 380 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-2000-6","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 2000 mm, Länge: 456 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-2000-7","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 2000 mm, Länge: 532 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-2000-8","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 2000 mm, Länge: 608 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-2000-9","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 2000 mm, Länge: 684 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-250-10","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 250 mm, Länge: 760 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-250-11","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 250 mm, Länge: 836 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-250-12","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 250 mm, Länge: 912 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-250-13","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 250 mm, Länge: 988 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-250-14","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 250 mm, Länge: 1064 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-250-15","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 250 mm, Länge: 1140 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-250-16","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 250 mm, Länge: 1216 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-250-17","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 250 mm, Länge: 1292 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-250-18","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 250 mm, Länge: 1368 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-250-19","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 250 mm, Länge: 1444 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-250-20","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 250 mm, Länge: 1520 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-250-22","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 250 mm, Länge: 1672 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-250-24","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 250 mm, Länge: 1824 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-250-26","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 250 mm, Länge: 1976 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-250-28","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 250 mm, Länge: 2128 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-250-30","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 250 mm, Länge: 2280 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-250-4","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 250 mm, Länge: 304 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-250-5","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 250 mm, Länge: 380 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-250-6","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 250 mm, Länge: 456 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-250-7","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 250 mm, Länge: 532 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-250-8","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 250 mm, Länge: 608 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-250-9","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 250 mm, Länge: 684 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-400-10","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 400 mm, Länge: 760 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-400-11","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 400 mm, Länge: 836 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-400-12","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 400 mm, Länge: 912 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-400-13","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 400 mm, Länge: 988 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-400-14","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 400 mm, Länge: 1064 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-400-15","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 400 mm, Länge: 1140 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-400-16","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 400 mm, Länge: 1216 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-400-17","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 400 mm, Länge: 1292 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-400-18","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 400 mm, Länge: 1368 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-400-19","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 400 mm, Länge: 1444 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-400-20","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 400 mm, Länge: 1520 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-400-22","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 400 mm, Länge: 1672 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-400-24","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 400 mm, Länge: 1824 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-400-26","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 400 mm, Länge: 1976 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-400-28","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 400 mm, Länge: 2128 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-400-30","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 400 mm, Länge: 2280 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-400-4","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 400 mm, Länge: 304 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-400-5","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 400 mm, Länge: 380 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-400-6","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 400 mm, Länge: 456 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-400-7","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 400 mm, Länge: 532 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-400-8","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 400 mm, Länge: 608 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-400-9","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 400 mm, Länge: 684 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-500-10","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 500 mm, Länge: 760 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-500-11","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 500 mm, Länge: 836 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-500-12","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 500 mm, Länge: 912 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-500-13","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 500 mm, Länge: 988 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-500-14","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 500 mm, Länge: 1064 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-500-15","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 500 mm, Länge: 1140 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-500-16","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 500 mm, Länge: 1216 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-500-17","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 500 mm, Länge: 1292 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-500-18","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 500 mm, Länge: 1368 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-500-19","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 500 mm, Länge: 1444 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-500-20","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 500 mm, Länge: 1520 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-500-22","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 500 mm, Länge: 1672 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-500-24","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 500 mm, Länge: 1824 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-500-26","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 500 mm, Länge: 1976 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-500-28","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 500 mm, Länge: 2128 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-500-30","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 500 mm, Länge: 2280 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-500-4","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 500 mm, Länge: 304 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-500-5","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 500 mm, Länge: 380 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-500-6","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 500 mm, Länge: 456 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-500-7","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 500 mm, Länge: 532 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-500-8","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 500 mm, Länge: 608 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-500-9","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 500 mm, Länge: 684 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-600-10","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 600 mm, Länge: 760 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-600-11","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 600 mm, Länge: 836 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-600-12","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 600 mm, Länge: 912 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-600-13","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 600 mm, Länge: 988 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-600-14","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 600 mm, Länge: 1064 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-600-15","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 600 mm, Länge: 1140 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-600-16","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 600 mm, Länge: 1216 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-600-17","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 600 mm, Länge: 1292 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-600-18","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 600 mm, Länge: 1368 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-600-19","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 600 mm, Länge: 1444 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-600-20","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 600 mm, Länge: 1520 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-600-22","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 600 mm, Länge: 1672 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-600-24","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 600 mm, Länge: 1824 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-600-26","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 600 mm, Länge: 1976 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-600-28","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 600 mm, Länge: 2128 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-600-30","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 600 mm, Länge: 2280 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-600-4","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 600 mm, Länge: 304 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-600-5","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 600 mm, Länge: 380 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-600-6","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 600 mm, Länge: 456 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-600-7","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 600 mm, Länge: 532 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-600-8","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 600 mm, Länge: 608 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-600-9","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 600 mm, Länge: 684 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-900-10","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 900 mm, Länge: 760 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-900-11","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 900 mm, Länge: 836 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-900-12","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 900 mm, Länge: 912 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-900-13","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 900 mm, Länge: 988 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-900-14","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 900 mm, Länge: 1064 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-900-15","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 900 mm, Länge: 1140 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-900-16","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 900 mm, Länge: 1216 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-900-17","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 900 mm, Länge: 1292 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-900-18","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 900 mm, Länge: 1368 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-900-19","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 900 mm, Länge: 1444 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-900-20","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 900 mm, Länge: 1520 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-900-22","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 900 mm, Länge: 1672 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-900-24","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 900 mm, Länge: 1824 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-900-26","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 900 mm, Länge: 1976 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-900-28","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 900 mm, Länge: 2128 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-900-30","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 900 mm, Länge: 2280 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-900-4","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 900 mm, Länge: 304 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-900-5","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 900 mm, Länge: 380 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-900-6","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 900 mm, Länge: 456 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-900-7","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 900 mm, Länge: 532 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-900-8","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 900 mm, Länge: 608 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C1-900-9","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C1, Höhe: 900 mm, Länge: 684 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-1200-10","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 1200 mm, Länge: 380 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-1200-12","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 1200 mm, Länge: 456 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-1200-14","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 1200 mm, Länge: 532 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-1200-16","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 1200 mm, Länge: 608 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-1200-18","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 1200 mm, Länge: 684 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-1200-20","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 1200 mm, Länge: 760 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-1200-6","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 1200 mm, Länge: 228 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-1200-8","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 1200 mm, Länge: 304 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-1600-10","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 1600 mm, Länge: 380 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-1600-12","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 1600 mm, Länge: 456 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-1600-14","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 1600 mm, Länge: 532 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-1600-16","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 1600 mm, Länge: 608 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-1600-18","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 1600 mm, Länge: 684 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-1600-20","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 1600 mm, Länge: 760 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-1600-6","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 1600 mm, Länge: 228 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-1600-8","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 1600 mm, Länge: 304 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-1800-10","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 1800 mm, Länge: 380 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-1800-12","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 1800 mm, Länge: 456 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-1800-14","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 1800 mm, Länge: 532 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-1800-16","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 1800 mm, Länge: 608 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-1800-18","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 1800 mm, Länge: 684 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-1800-20","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 1800 mm, Länge: 760 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-1800-6","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 1800 mm, Länge: 228 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-1800-8","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 1800 mm, Länge: 304 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-2000-10","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 2000 mm, Länge: 380 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-2000-12","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 2000 mm, Länge: 456 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-2000-14","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 2000 mm, Länge: 532 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-2000-16","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 2000 mm, Länge: 608 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-2000-18","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 2000 mm, Länge: 684 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-2000-20","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 2000 mm, Länge: 760 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-2000-6","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 2000 mm, Länge: 228 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-2000-8","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 2000 mm, Länge: 304 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-250-10","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 250 mm, Länge: 380 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-250-12","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 250 mm, Länge: 456 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-250-14","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 250 mm, Länge: 532 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-250-16","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 250 mm, Länge: 608 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-250-18","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 250 mm, Länge: 684 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-250-20","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 250 mm, Länge: 760 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-250-22","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 250 mm, Länge: 836 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-250-24","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 250 mm, Länge: 912 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-250-26","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 250 mm, Länge: 988 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-250-28","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 250 mm, Länge: 1064 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-250-30","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 250 mm, Länge: 1140 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-250-6","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 250 mm, Länge: 228 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-250-8","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 250 mm, Länge: 304 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-400-10","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 400 mm, Länge: 380 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-400-12","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 400 mm, Länge: 456 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-400-14","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 400 mm, Länge: 532 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-400-16","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 400 mm, Länge: 608 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-400-18","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 400 mm, Länge: 684 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-400-20","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 400 mm, Länge: 760 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-400-22","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 400 mm, Länge: 836 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-400-24","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 400 mm, Länge: 912 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-400-26","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 400 mm, Länge: 988 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-400-28","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 400 mm, Länge: 1064 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-400-30","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 400 mm, Länge: 1140 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-400-6","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 400 mm, Länge: 228 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-400-8","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 400 mm, Länge: 304 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-500-10","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 500 mm, Länge: 380 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-500-12","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 500 mm, Länge: 456 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-500-14","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 500 mm, Länge: 532 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-500-16","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 500 mm, Länge: 608 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-500-18","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 500 mm, Länge: 684 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-500-20","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 500 mm, Länge: 760 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-500-22","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 500 mm, Länge: 836 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-500-24","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 500 mm, Länge: 912 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-500-26","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 500 mm, Länge: 988 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-500-28","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 500 mm, Länge: 1064 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-500-30","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 500 mm, Länge: 1140 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-500-6","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 500 mm, Länge: 228 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-500-8","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 500 mm, Länge: 304 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-600-10","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 600 mm, Länge: 380 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-600-12","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 600 mm, Länge: 456 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-600-14","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 600 mm, Länge: 532 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-600-16","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 600 mm, Länge: 608 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-600-18","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 600 mm, Länge: 684 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-600-20","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 600 mm, Länge: 760 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-600-22","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 600 mm, Länge: 836 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-600-24","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 600 mm, Länge: 912 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-600-26","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 600 mm, Länge: 988 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-600-28","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 600 mm, Länge: 1064 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-600-30","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 600 mm, Länge: 1140 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-600-6","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 600 mm, Länge: 228 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-600-8","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 600 mm, Länge: 304 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-900-10","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 900 mm, Länge: 380 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-900-12","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 900 mm, Länge: 456 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-900-14","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 900 mm, Länge: 532 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-900-16","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 900 mm, Länge: 608 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-900-18","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 900 mm, Länge: 684 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-900-20","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 900 mm, Länge: 760 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-900-22","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 900 mm, Länge: 836 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-900-24","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 900 mm, Länge: 912 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-900-26","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 900 mm, Länge: 988 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-900-28","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 900 mm, Länge: 1064 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-900-30","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 900 mm, Länge: 1140 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-900-6","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 900 mm, Länge: 228 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["C2-900-8","\"\"","HG-TEC Climaster Hygiene-Heizkörper","Typ C2, Höhe: 900 mm, Länge: 304 mm","Stck",0,"","","","","CLIMA","CLIMASTER","","","N"]
["EPC12","\"\"","Elektroheizpatrone Typ EPC12","Nennleistung 1200 W, Einbaulänge 920 mm","Stck",0,"","","","","","HEIZPATRONE","","","N"]
["EPC15","\"\"","Elektroheizpatrone Typ EPC15","Nennleistung 1500 W, Einbaulänge 1100 mm","Stck",0,"","","","","","HEIZPATRONE","","","N"]
["EPC20","\"\"","Elektroheizpatrone Typ EPC20","Nennleistung 2000 W, Einbaulänge 1250 mm","Stck",0,"","","","","","HEIZPATRONE","","","N"]
["EPC30","\"\"","Elektroheizpatrone Typ EPC30","Nennleistung 300 W, Einbaulänge 350 mm","Stck",0,"","","","","","HEIZPATRONE","","","N"]
["EPC60","\"\"","Elektroheizpatrone Typ EPC60","Nennleistung 600 W, Einbaulänge 550 mm","Stck",0,"","","","","","HEIZPATRONE","","","N"]
["EPC90","\"\"","Elektroheizpatrone Typ EPC90","Nennleistung 900 W, Einbaulänge 710 mm","Stck",0,"","","","","","HEIZPATRONE","","","N"]
["FBT","\"\"","Fensterbankträger für C1 und C2","verstellbar","Stck",0,"","","","","","FENSTERBANKTRÄG","","","N"]
["SAS1","\"\"","Verchromtes T-Stück 1/2\"","für Mixbetrieb","Stck",0,"","","","","","T-STÜCK","","","N"]
["STK","\"\"","Standkonsole, höhenverstellbar","für Typ C1 und C2","Stck",0,"","","","","","KONSOLE","","","N"]
["TH810T","\"\"","Raumthermostat Typ TH 810T mit","programmierbarer Zeitsteuerung","Stck",0,"","","","","","THERMOSTAT","","","N"]
["WKC1","\"\"","Wandkonsole für Typ C1","inkl. Schrauben und Dübel","Stck",0,"","","","","","KONSOLE","","","N"]
["WKC2","\"\"","Wandkonsole für Typ C2","inkl. Schrauben und Dübel","Stck",0,"","","","","","KONSOLE","","","N"]
["ZSG101","\"\"","Raumregler/Zentralsteuergerät","Tag- und Nachtabsenkung","Stck",0,"","","","","","RAUMREGLER","","","N"]